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	1. 
Name of the firms / manufacturers/vendor: ……………………………………………………

2. 
Name and Designation of

Authorized Signatory:

………………………………………………………………..

3. 
Communication Address: 

……………………………………………..…………………


 



            ………………………………………………………………..

4.
 Phone No. / Mobile No. 

………………………………………….……………………

5.
Fax:




……………………………………….………………………

6. 
E-Mail ID: 



…………………………………….…………………………

7. 
PAN NO: 



…………………………………….…………………………

8. 
GST No:

     
              …………………………………………………….………..

9.
Type of firm:


Individual 
      Partnership
              Company.
     Co-operative Society


/Proprietorship



/Pvt Ltd/Ltd









10.
Credential certificate /POs from reputed institutions:…………………………………….

11.
Income Tax Return as on current dates:
………………………………………………………..

12.
GST No & Certificate:………………………………………..

13.
Valid Registration / License Certificate ……………………………………………………………. 
14.
Bank Details with cancel cheque:


Name of the Bank:………………………………………Branch Name:
……………………


Type of Account:…………………… Account No:………………..IFS Code:……………………

(Bal Raksha Bharat - Save the Children reserves right to call for proof / documents for verifications)

Copies of all above documents are attested, company sealed & submitted along with this letter.

UNDERTAKING

· I, the undersigned certify that I have gone through the terms and conditions mentioned in the bidding document and undertake to comply with them.

· The rates quoted by me in two separate sealed envelopes (Technical & Financials are valid till ____________and binding upon me for the above WASH civil construction and repair work, in Nellore District, Andra Pradesh. 
· I/We give the rights to the Bal Raksha Bharat - Save the Children to cancel the bids in case of breach of conditions of Contract.

Signature of the Authorized Signatory

Designation:

(Office seal of the Bidder) 

Date:  ………..…………  

Place: ………………….


General Details of Bidder 
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		Terms of Reference

Civil Repair and refurbishment of schools based on the need assessment & awareness on WASH and its importance to the students





About Bal Raksha Bharat 



Bal Raksha Bharat (Also known as Save the Children) is a global non-profit organization, founded in 1919 as a response to the condition in Europe immediately following the First World War, is a federation of 29 members with similar vision, mission, and values for children, working in more than 120 countries to form a truly international movement for children. In 2008, Bal Raksha Bharat (Save the Children) registered in Indian as ‘Bal Raksha Bharat’. Today Bal Raksha Bharat (Save the Children) is India’s leading independent child rights organization. Presently, we have presence across 16 states of India and have impacted the lives of more than 14 million children since 2008.



About Project:

To improve the safety, hygiene, functionality and overall learning environment in 5 Government schools by strengthening WASH facilities and undertaking essential infrastructure repair, renovation and refurbishment works.



Background: Bal Raksha Bharat with support from SEIL Energy India Limited has implemented projects on Education theme in Government schools Nellore in the year 2022 -2024. The programmes were focussed on providing access to quality education to the children and strengthening of capacities of the teaching staff. 



Proposed Project Rationale: The proposed intervention aims to create safe, hygienic, inclusive and child-friendly learning environments by strengthening essential school infrastructure and Water, Sanitation and Hygiene (WASH) facilities in Five schools. 

The identified 05 schools serving children from economically and socially vulnerable communities face challenges related to ageing and poorly maintained infrastructure. These include deteriorated toilets, damaged flooring and wall tiles, inadequate water and sanitation facilities, unsafe electrical systems, no painting, damaged doors/windows, cracks and dampness in walls and ceilings, and other infrastructure lacks. These conditions can adversely affect children's health, safety, dignity, attendance and overall learning experience, particularly for girls and adolescent students.

This proposal aims to undergo need-based repair, renovation and refurbishment based on systematic school-level infra technical assessments. The programme will prioritize critical infrastructure and WASH gaps and ensure that the investments result in visible, functional, safe and sustainable improvements. The intervention will also promote greater ownership among school management, teachers, School Management Committees (SMCs) and other stakeholders, with emphasis on regular maintenance and sustainability of the improved facilities.

Common challenges observed in schools:

· Damaged or poorly maintained toilets.

· Broken or deteriorated flooring and wall tiles.

· Plumbing and water supply deficiencies.

· Damaged doors, windows and other civil structures.

· Unsafe electrical wiring, switches, lights and fans.

· Inadequate finishing of class rooms 

· Poor sanitation and hygiene conditions.

Project Goal: To improve the safety, hygiene, functionality and overall learning environment of schools by strengthening WASH facilities and undertaking essential infrastructure repair, renovation and refurbishment works.

Project Objectives: 

1. Improve access to safe, functional and hygienic toilet facilities. 

2. Repair and renovate school infrastructure. 

3. Improve flooring, wall surfaces and tiling ias required in the respective schools. 

4. Upgrade electrical installations to improve safety and functionality. 

5. Improve class rooms through painting, finishing and essential civil works as per the technical assessment. 

6. Improve the safety and usability of classrooms, corridors and common areas. 

Details of 5 Schools:

		Sr No

		School Name

		Boys

		Girls

		School Staff



		1

		ZPHS – MV Palem

		150

		170

		10



		2

		MPP UP School- Mandapam

		16

		13

		2



		3

		UPS Pynapuram-DH Wada

		30

		20

		3



		4

		MPP UP School-Varakavipudi (upgraded to ZPHS)

		116

		108

		12



		5

		ZPHS – Eduru

		170

		160

		25



		TOTAL

		482

		471

		52







* The above is the tentative school list and permissions will be taken from the Government Education Department before start of work. Any change in the above school list shall be intimated to SEIL and due approval shall be taken from the Government Education Department.



1. Complete all the infrastructure work neatly



2. Excavation work: Excavation in all types of soil including dense soil, disintegrated/weathered/soft rock for  footings of Retaining walls, catchpits, Lift pits, trenches for drains, etc.,by manual means where it is not possible to excavate by machines or mechanical means including excavation for levelling, dressing the edges, all leads and lifts including back filling in layers of 150mm with watering and compaction, dewatering of both ground and surface water, removal of slurry generated while excavation and keeping the area free of water with necessary shoring, strutting, required for keeping earth in position etc. Rate to include disposing the excess earth and spreading in layers to the required levels within the site wherever specified and carting away outside the site to the designated areas identified by the local authorities. Brick work: Providing & constructing with Hallow brick masonry



3. Filling: providing and filling available excavated earth (excluding rock) in sides of foundations, trenches, footings, in plinth, behind retaining walls, under the floors or in  ramp  etc.,  in layers  not  exceeding  20cms.  in depth, compacting each deposited layer by ramming after watering with all leads and lifts including cost of all labour complete as per specifications and as directed by Architects and Engineer-in-Charge.



4. SSM: Providing and constructing granite / trap/ basalt size stone masonry in foundation with cement mortar, stone hammered dressed in courses not less than 20 cms high, bond stones at 2m. apart in each course including cost of materials, labour, curing complete as per specifications 



5. Block work: Providing & constructing with Concrete block masonry 200mm thick in superstructure at all levels and heights with approved quality Hallow brick of minimum crushing strength 50 kgs/sqcm, in CM 1:6 including raking the joints neatly to a depth of 12mm, curing, scaffolding, with all leads and lifts and as directed by STC Engineer in charge. etc. complete.



6. Wall Plastering: Providing the surface and plaster  the walls with cement mortar 1:6 , 15 mm thick , smooth finished to line and plumb with lime rendering at all levels rounding of corners wherever required complete with necessary scaffolding, curing etc, complete.including lead and lifts hydrating the lime for 24 hours before starting of work.



7. Ceiling Plastering: Providing the surface and plaster  the walls with cement mortar 1:6 , 15 mm thick , smooth finished to line and plumb with lime rendering at all levels rounding of corners wherever required complete with necessary scaffolding, curing etc, complete.including lead and lifts hydrating the lime for 24 hours before starting of work.



8. Painting: Providing one primer coat and two coats of Apex Exterior paint (Asian Paints) or  equivalent, as  per  approved  shade  &  manufacture  after  thoroughly sand papering the surfaces, removing the dust, dirt, repairing dents, holes, cracks, etc.,  applying  a  coat  of  primer  including  labour,  scaffolding  at  all  levels  with primer & putty etc., complete



9. Ceiling painting: Prepare the surface of ceiling., and apply wall putty for the ceiling and apply over one coat of appropriate primer, including preparing the surface after thoroughly cleaning the surface to remove all dirt, dust and foreign matter, cost of materials, labour complete as per specifications, scaffolding etc., complete. The rate shall include for finishing the painting to obtain an even and uniform shade as directed by the STC Engineer.  



10. Plain cement concrete: Providing and laying plain cement concrete (PCC) 1:4:8 for flooring with smooth finishing using graded granite aggregate of 12 mm and down size, provide thickness upto 4" and it including martials, labours, manual mixing/machine mixing, compacted by wooden or cast iron rammers, curing etc., complete.



11. Floor Tiles work: floor tile Providing and laying first quality ceramic tiles 300x300mm of approved colour, make and set in cement mortor, 20mm thick including pointing with tinted white cement to match the colour of tiles. Rate to include for laying tiles of approved size to the pattern as directed by the organization including curing, acid wash etc., complete.  the rate shall include for POP coating over polythene sheet for protection of the polished floor till handing over the building.      



12. Wall Tiles work: Providing and laying wall dadooing upto 5' ht , first  quality  Vitrified Tiles  of   approved  colour, make  300x 400mm Glossy finish of approved colour, make and set in cement mortor, 20mm thick including pointing with tinted white cement to match the colour of tiles. Rate to include for laying tiles of approved size to the pattern as directed by the organization including curing, acid wash etc., complete.  the rate shall include for POP coating over polythene sheet for protection of the polished wall till handing over the building.  



13. RCC: Providing & laying controlled reinforced cement concrete conforming to grades as specified  in  (IS  456  -  2000)  as  per  specifications  at  all  levels  and  location including transporting through transit mixer, of specified grade using 43/53 grade cement,   20mm  and  down  size  coarse  graded  machine  crushed  hard  stone aggregate including designing the mix, batching, mechanical mixing, transporting, pumping  and  placing  at  all  levels  of  all  shapes  and  sizes  including  laying  to required  slope,  compaction  using  vibrators,  curing  and  finishing  smooth  as required for the following RCC Structural or other elements, scaffolding, hacking the  exposed  concrete  surface  wherever  required.   Cost to include appropriate dewatering wherever necessary to lay the concrete, cost of all materials, labours all lead and lifts, tools, plant and machinery, hire and fuel charges and all other incidental charges etc., all as per specifications, drawings and as directed, but excluding steel reinforcement,  IRC  Mesh,  insert  plates,  which  will  be  paid separately under relevant items, making holes or cutting. The rate shall include for providing  recess  to  walls  or  columns,  sleeves  in  slabs,  construction  joints  sunk slabs, cantilever slabs, making holes or cutting form work for taking out Electrical conduits  or dowels for column to Brick work, to the required shape, size, slope shown in drawings for the following items of work. (Rate Including Shuttering).



14. Reinforcement steel: Supplying and fixing reinforcement for R.C.C.  In  all  items  works  including transporting, decoiling, cutting, straightening bending and placing in position at all levels and binding with approved gauge binding wire. The rate shall include cost of  binding  wire, chairs,  spacers  which  will not  be measured  separately  for payment.  Quantity of steel as per drawing and with authorized overlaps only shall be measured and paid for.  High yield strength deformed bars conforming to Yst 415 N/mm2 as per IS 1786



15. MS door: Providing & fixing iron door MS iron sheet heavy duty 16SGW, iron angle frame 35X35mm and internal cross support to sheet, interlocking together their entire length & joint together at ends lock, handle, hinges with two l drop etc complete with two coat of metal primer and two coat of enamel paint as per the direction of STC Engineer incharge.



16. MS Ventilator: Providing and fixing of new Ventilator with suitable angles with Fe415 guage. Rate shall includes removal of debrise and disposal of materials during removal and material cost and labour cost (fabrication and fixing) and also complete with one coat primer and 2 coat enamel paint as per the direction of STC Engineer incharge.



17. Toilet water closet: Providing and fixing water closet squatting pan (Indian type W.C. pan) with 100 mm sand cast Iron P or S trap, Complete with all fittings and fixtures complete, including cutting and making good the walls and floors wherever required.



18. Girls Urinals: Providing and fixing white squatting urinal plate with necessary water connection and septic tank connection. Cost shall include all necessary items requires for water connection (L-bow, T joint etc). All PVC pipe lines connections and other pipe line repairs. (PVC pipe thickness=3/4") (Rate shall includes 1" Kadapa stone partition between urinals) (Rate shall include health faucet which depends on quatity of urinals)



19. Boys Urinals: Providing and laying Single half stall urinal with 5 liter white P.V.C, with necessary water connection and septic tank connection. Cost shall include all necessary items requires for water connection (L-bow, T joint etc). All PVC pipe lines connections and other pipe line repairs. (PVC pipe thickness=3/4") (Rate shall include tiles work if necessary while placing the urinals if damaged the existing tile work)



20. Wash Basin: Providing and fixing Flat back wash basin of size 405X325 mm with C.I. brackets, 15 mm C.P. brass pillar taps, 32 mm C.P. brass waste of standard pattern, including painting of fittings and brackets, cutting and making good the walls wherever require: Cost shall includes water connections and outlet connection with all necessary items requires for water connection (L-bow, T joint etc). All PVC pipe lines connections and other pipe line repairs. (PVC pipe thickness=3/4") with wash basin steel tap.



21. OHT: Providing 500 liters Over head tank (OHT) to the School. Cost shall include installation, labour cost and etc., Complete



22. Water Connection: Provide proper water Connection  from motor to OHT and toilet. Cost shall include all necessary items requires for water connection (Elbow, T joint etc). All CPVC pipe lines connections and other pipe line repairs. (PVC pipe thickness=3/4").



23. Plain cement concrete: Providing and laying plain cement concrete (PCC) 1:4:8 for flooring with smooth finishing using graded granite aggregate of 12 mm and down size, provide thickness upto 4" and it including martials, labours, manual mixing/machine mixing, compacted by wooden or cast iron rammers, curing etc., complete. (Ramp)



24. Septic tank: Construction of new septic tank  using 6 no's precast RCC rings, with caps(self casted RCC cap with 50.8 mm thick) drainage line from toilet to septic tank to make it functional and complete with filling 40mm jelly around the rings till 4feet height.  (4ft dia, 7 ft depth, 1ft Above GL) (Scope includes Excavations, Backfill, civil works (1 cement bag), plumbing works, labour charges, req material, req machinery, site cleaning and all other material, manpower required to make it functional).



25. Providing and Fabricating MS Railing for Ramp as shown in drawings.

26. Providing 4" PVC pipe for septic tank connection from the toilet.

27. Providing SS grade 304 Soap Stand

28. Providing and fixing Cockroach trap

29. Providing and fixing Long body tap with all necessary fixtures.

30. MS mesh for windows and ventilators: Providing and fixing 1"x1" square MS welded wire mesh for windows/Ventilators with all necessary fixture and finishing the same with one coat of zinc chromate primer and two coats of enamel paint of approved make. The M.S. Grill is with following members: (a) 25x6mm Brite Flat as vertical member; (b) 10mm square brite horizontal bar punched through the flat Rate shall include material cost, labour cost, cutting charges shifting, welding etc., Complete as per the STC engineer in charge (Option mosquito mesh as per engineer suggestion)



Requirement: Bal Raksha Bharat Karnataka office is looking for a competent individual or agency to undertake the assignment who will be able to take the feedback from Bal Raksha Bharat. 



Terms & Conditions; 

· Individual consultant or agency must have previous experience in dealing with the same nature of work of construction/renovation/painting/illustration work. 

· The infra work should not be compromised on quality. The work should be strong that will last long unless there is some natural or man-made destruction or wall loose its strength due to some internal unknown factors. 

· High quality materials to be used as per specifications given by Bal Raksha Bharat.

· The appearance of the work should be noticeably visible and captivating 

· Bal Raksha Bharat will provide point of contact in advance before starting the assignment on ground. 

· Contractor shall coordinate with the Engineer-in-charge and accommodate necessary adjustments or changes during execution, without additional cost unless approved.

· GST certificate is expected in case of falling within the financial framework of Indian Taxation System. 

· Contractor will be required to adhere to the Child Safeguarding Policy and ethnical guidelines.

· Background checks will be undertaken for all applicants

Support from Bal Raksha Bharat: Bal Raksha Bharat will will coordinate with the concerned School Head teachers and facilitate opening of the schools during the work. Will also provide the address and will assign one person in case of any support required. 



Selection Process: Bal Raksha Bharat procurement and program committee would like to review all the submitted proposals and prefer an agency which has competencies, competitive financial submission, deliver in no time, previous satisfying experience with other development agencies and Bal Raksha Bharat and finally understand the Child Rights.

[bookmark: _Hlk174894163]

Location: Nellore District, Andra Pradesh





Scope of the work:



The vendor must work in project schools as per the specifications outlined above as part of ToR as per the terms and conditions given below:







[bookmark: _Toc34211485][bookmark: _Toc45802795][bookmark: _Toc62144589][bookmark: _Toc62144735]Reporting Procedure:

· Inception report to be developed that contains detailed work plan

· Vendors will report to the Project Lead, Civil Engineer (Bal Raksha Bharat) about the progress of work and is obliged to do the work assigned by the organization for construction and renovation work. 

· The Vendor has to maintain the daily activity report and also needs to submit the weekly report to review the status.  

Support from Save the Children: 

· BOQ will be shared with Vendors

· Documents related to the project will be shared with Vendors for making him/her to have better understanding towards the assignment

· Facilitate consultant for developing route map 

· Coordinating with schools for field visits with the help of ASF

Time frame: 

The contractor shall commence work from the date of work order and complete the project within the timeframe about 90 days agreed upon in the contract, ensuring timely delivery without unnecessary delays.  

The vendor should abide by the timings of the opening and closing of the center. 



Terms of Payment:



Tax deductions will apply to the fees of the Consultant in accordance with the prevailing Income Tax legislation/policy of the Government of India



Payment Schedule: 

· Advance at the time of agreement: 40%

· After completion of the 50% work: 30

· After sharing final report: 30%



 Ethics, child safeguarding and Code of Conduct:



· As the selected Vendors/Agency will be working on behalf of Save the Children, they will be required to adhere to the Child Safeguarding Policy and ethical guidelines. The Consultant/Agency and the study team engaged in the review will receive orientation on and sign Save the Children’s Child Safeguarding Policy. Background checks will be undertaken for all applicants. 

· The Vendor/Consultant/Agency will make clear to all participating stakeholders especially children of all ages that they are under no obligation to participate in the process. All participants will be assured that there will be no negative consequences if they choose not to participate. 

· As the shortlisted Consultant/Agency needs to interact with children s/he needs to sign and abide by Save the Children’s Child Safeguarding Policy. 



Support to be provided by Bal Raksha Bharat team: 



[bookmark: _Toc29483122][bookmark: _Toc45802797]SC Staff in the State and National Support Office will extend the required support during the work in terms of information/approvals required; an appropriate project staff will be assigned to support the Vendor’s team.
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SUMMARY

		SEIL PROJECT

		CIVIL WORKS

		SL.NO		DISTRICT		NAME OF SCHOOL		LINK		AMOUNT

		1		NELLORE		ZPHS – MV Palem		MV Palem'!A1		- 0

		2		NELLORE		MPP UP School- Mandapam		GUDURU MANDALAM'!A1		- 0

		3		NELLORE		UPS Pynapuram-DH Wada		PYNAPURAM!A1		- 0

		4		NELLORE		MPP UP School-Varakavipudi (upgraded to ZPHS)		VARAKAVIPUDI!A1		- 0

		5		NELLORE		ZPHS – Eduru		EDURU!A1		- 0

		TOTAL								- 0





MV Palem

		BAL RAKSHA BHARAT

		MV PALEM

		R0

		Item		Description		Brands		Unit		No's		No's		L		B		D		Qty		Rate		Amount		Remarks

		A		CIVIL WORKS IN BOYS TOILET

		1		Water proofing the Roof slab : The first method consists of water proofing by surface method of average thickness 2" with waterproof admixture as per manufacturer's specification approved by Consultants with a minimum Guarantee period of 10 years. Cost to include – Cement slurry with waterproofing compound applied over the surface after cleaning the surface - Laying of brick coba to necessary gradient and joints filled with CM 1:4 with water proofing compoundCost to include the treatment along parapet,treatment to construction joints,pressure grouting of damp areas using cementitious grouting etc, and no extra measurements shall be accounted for the parapet treatment with Curing the entire surface for  a minimum  period of seven days.  (CLEANING AND CHEMICAL COATING)		Birla Opus ALLDRY/JSW I BLOCK WATERSTOP  ROOF COAT		Sft		1		1		23		9				207				- 0

		2		Providing ACID WASH for toilet		ROFF		Ltrs		1		10								10				- 0

		3		Painting (Internal and External): Providing two coats  of Apex paint (Asian Paints)  or  equivalent  ,as  per  approved  shade  &  manufacture  after  thoroughly sand papering the surfaces, removing the dust, dirt, repairing dents, holes, cracks, etc.,  applying  a  coat  of  primer  including  labour,  scaffolding  at  all  levels  with primer & putty etc., complete. (Including Ceiling)		Asian/ Birla		Sft		1				64				10		891.24

				Inner walls				Sft		1				80				10		800

				Deductions

				Doors				Sft		-1		1		3				7		-21

				Ventilators				Sft		-2		4		2		2				-32

				Total				Sft												1638.24				- 0

		4		Enamel Paints to Doors, Windows, Grills, Metallic Surfaces,
Walls : Providing & applying Enamel Paints to Doors, Windows, Grills, Metallic Surfaces, walls, etc. Removing, scrapping & cleaning the
existing enamel paint on doors, windows, grills, metallic surfaces, etc.
paint by scrapping, sand papering and scrubbing. Then first coat of
primer to be applied. After this necessary leveling shall be done with
putty & second primer coat shall be applied. and The enamel paint of approved shade shall be applied in minimum 3coats (finishing paint) including scaffolding, cleaning the floors, fittings, furniture's, ladders, glasses, removing of debris out of the compound etc. complete as per the instructions of the Engineer.		Asian/Birla		Sft

				Doors				Sft		1		1		3				7		21

				Ventilators				Sft		2		4		2		2				32

				Total				Sft												53				- 0

		5		4" PVC pipe for drainage connection		Ashirvad		Rft		1				100						100				- 0

		6		Providing 3" L bow for Connection		Ashirvad		No's		1				100						100				- 0

		7		OHT: Providing 1000 litres Over head tank (OHT) to the School. Rate shall include installation (tank nipple, union, adaptor), labour cost and etc., Complete		Ashirvad		Liters		1000										1000				- 0

		8		Water Connection: Provide proper water Connection  from motor to OHT. Cost shall include all necessary items requires for water connection(Elbow, T joint etc). All CPVC pipe lines connections and other pipe line repairs. (CPVC pipe dia=3/4"). 		Ashirvad		Rft		1				200		 		 		200				- 0

		9		Providing and Installing safety grill for Motor near the Boys toilet		Material Available in Market 		lumpsum		1										1				- 0

		10		MS door: Providing and fixing 1mm thick M.S. sheet door with frame of 40x40x6 mm angle iron and 3 mm M.S. gusset plates at the junctions and corners, all necessary fittings complete, including applying a priming coat of approved steel primer. Using M.S. angels 40x40x6 mm for diagonal braces including cost of materials, labour, usage charges of machinery complete as per specifications and as per directions of the Engineer-in- Charge.		MS Engineering works		Sft		1		2		4				7		56				- 0

		11		Plain cement concrete: Providing and laying plain cement concrete(PCC) 1:4:8 for flooring with smooth finishing using graded granite aggregate of 12 mm and down size, provide thickness upto 4" and it including matrials, labours, manual mixing/machine mixing, compacted by wooden or cast iron rammers, curing etc., complete. (Including RCC)		ACC/ Birla Super, Ultratech,Materials available in Market		Cft		1		1		100		5		0.3		150				- 0		Pathway 

		12		Urinals: Providing and laying Single half stall urinal with 5 litre white Ceramic of Niagara N C0579 (280 x 335 x 465mm), with necessary water connection and septic tank connection. Cost shall include all necessary (urinal connection pipe (Hose pipe, Spreader urinal set)) items requires for water connection(L-bow, T joint etc). All PVC pipe lines connections and other pipe line repairs. (PVC pipe dia=2").		Parryware		No's		1		4								4				- 0

		13		Providing 2" PVC pipe for urinal waste water to Septic tank connection. Cost shall include all necessary items requires for connection(Elbow, T etc). All PVC pipe lines connections and other pipe line repairs. (PVC pipe dia=2"). 		Ashirvad		Rft		1				50						50				- 0

		14		Wall Plastering: Providing the surface and plaster  the walls with cement mortar 1:6 , 15 mm thick , smooth finished to line and plumb with lime rendering at all levels rounding of corners wherever required complete with necessary scaffolding, curing etc, complete.including lead and lifts hydrating the lime for 24 hours before starting of work.		Ultratech,ACC,Birla super, 		Sft		1		1		10		10				100				- 0		Touchup works

		Sub Total for Civil works in Boys toilet																						- 0



		B		CIVIL WORKS IN GIRLS TOILET

		1		Water proofing the Roof slab : The first method consists of water proofing by surface method of average thickness 2" with waterproof admixture as per manufacturer's specification approved by Consultants with a minimum Guarantee period of 10 years. Cost to include – Cement slurry with waterproofing compound applied over the surface after cleaning the surface - Laying of brick coba to necessary gradient and joints filled with CM 1:4 with water proofing compoundCost to include the treatment along parapet,treatment to construction joints,pressure grouting of damp areas using cementitious grouting etc, and no extra measurements shall be accounted for the parapet treatment with Curing the entire surface for  a minimum  period of seven days.  (CLEANING AND CHEMICAL COATING)		Birla Opus ALLDRY/JSW I BLOCK WATERSTOP  ROOF COAT		Sft		1		1		23		9				207				- 0

		2		MS door: Providing and fixing 1mm thick M.S. sheet door with frame of 40x40x6 mm angle iron and 3 mm M.S. gusset plates at the junctions and corners, all necessary fittings complete, including applying a priming coat of approved steel primer. Using M.S. angels 40x40x6 mm for diagonal braces including cost of materials, labour, usage charges of machinery complete as per specifications and as per directions of the Engineer-in- Charge.		MS Engineering works		Sft		1		2		4				7		56				- 0

		3		4" PVC pipe for drainage connection		Ashirvad		Rft		1				100						100				- 0

		4		Providing 3" L bow for Connection		Ashirvad		No's		1				100						100				- 0

		5		OHT: Providing 1000 litres Over head tank (OHT) to the School. Rate shall include installation (tank nipple, union, adaptor), labour cost and etc., Complete		Ashirvad		Liters		1000										1000				- 0

		6		Water Connection: Provide proper water Connection  from motor to OHT. Cost shall include all necessary items requires for water connection(Elbow, T joint etc). All CPVC pipe lines connections and other pipe line repairs. (CPVC pipe dia=3/4"). 		Ashirvad		Rft		1				200		 		 		200				- 0

		7		Providing ACID WASH for toilet		ROFF		Ltrs		1		10								10				- 0

		8		Painting (Internal and External): Providing two coats  of Apex paint (Asian Paints)  or  equivalent  ,as  per  approved  shade  &  manufacture  after  thoroughly sand papering the surfaces, removing the dust, dirt, repairing dents, holes, cracks, etc.,  applying  a  coat  of  primer  including  labour,  scaffolding  at  all  levels  with primer & putty etc., complete. (Including Ceiling)		Asian/ Birla		Sft		1				64				10		891.24

				Inner walls				Sft		1				80				10		800

				Deductions

				Doors				Sft		-1		1		3				7		-21

				Ventilators				Sft		-2		4		2		2				-32

				Total				Sft												1638.24				- 0

		9		Enamel Paints to Doors, Windows, Grills, Metallic Surfaces,
Walls : Providing & applying Enamel Paints to Doors, Windows, Grills, Metallic Surfaces, walls, etc. Removing, scrapping & cleaning the
existing enamel paint on doors, windows, grills, metallic surfaces, etc.
paint by scrapping, sand papering and scrubbing. Then first coat of
primer to be applied. After this necessary leveling shall be done with
putty & second primer coat shall be applied. and The enamel paint of approved shade shall be applied in minimum 3coats (finishing paint) including scaffolding, cleaning the floors, fittings, furniture's, ladders, glasses, removing of debris out of the compound etc. complete as per the instructions of the Engineer.		Asian/Birla		Sft

				Doors				Sft		1		1		3				7		21

				Ventilators				Sft		2		4		2		2				32

				Total				Sft												53				- 0

		Sub Total for Civil works in Girls toilet																						- 0



		C		CIVIL WORKS 

		1		Water proofing the Roof slab : The first method consists of water proofing by surface method of average thickness 2" with waterproof admixture as per manufacturer's specification approved by Consultants with a minimum Guarantee period of 10 years. Cost to include – Cement slurry with waterproofing compound applied over the surface after cleaning the surface - Laying of brick coba to necessary gradient and joints filled with CM 1:4 with water proofing compoundCost to include the treatment along parapet,treatment to construction joints,pressure grouting of damp areas using cementitious grouting etc, and no extra measurements shall be accounted for the parapet treatment with Curing the entire surface for  a minimum  period of seven days.  (CLEANING AND CHEMICAL COATING)		Birla Opus ALLDRY/JSW I BLOCK WATERSTOP  ROOF COAT		Sft		1		1		40		10				400				- 0

		2		MS door: Providing and fixing 1mm thick M.S. sheet door with frame of 40x40x6 mm angle iron and 3 mm M.S. gusset plates at the junctions and corners, all necessary fittings complete, including applying a priming coat of approved steel primer. Using M.S. angels 40x40x6 mm for diagonal braces including cost of materials, labour, usage charges of machinery complete as per specifications and as per directions of the Engineer-in- Charge.		MS Engineering works		Sft		1		5		4				7		140				- 0		One door for Classroom

		3		4" PVC pipe for drainage connection		Ashirvad		Rft		1				100						100				- 0

		4		Providing 3" PVC pipe for drainage connection		Ashirvad		No's		1				100						100				- 0

		5		OHT: Providing 1000 litres Over head tank (OHT) to the School. Rate shall include installation (tank nipple, union, adaptor), labour cost and etc., Complete		Ashirvad		Liters		1000										1000				- 0

		6		Providing and fixing 1 HP motor with Proper Elctricity Connection 		Sharp/ Texmo		No's		1										1				- 0

		6		Water Connection: Provide proper water Connection  from motor to OHT. Cost shall include all necessary items requires for water connection(Elbow, T joint etc). All CPVC pipe lines connections and other pipe line repairs. (CPVC pipe dia=3/4"). 		Ashirvad		Rft		1				200		 		 		200				- 0

		7		Providing ACID WASH for toilet		ROFF		Ltrs		1		20								20				- 0

		8		Providing and Laying RCC slab for existing septic tank made with Reinforcement steel and M25 grade concrete mix and complete.		Ultratech,ACC,Birla super, 		Sqft		1				5		4				20				- 0

		9		Wall Plastering: Providing the surface and plaster  the walls with cement mortar 1:6 , 15 mm thick , smooth finished to line and plumb with lime rendering at all levels rounding of corners wherever required complete with necessary scaffolding, curing etc, complete.including lead and lifts hydrating the lime for 24 hours before starting of work.		Ultratech,ACC,Birla super, 		Sft		1		1		10		10				100				- 0		Touchup works

		10		Plain cement concrete: Providing and laying plain cement concrete(PCC) 1:4:8 for flooring with smooth finishing using graded granite aggregate of 12 mm and down size, provide thickness upto 4" and it including matrials, labours, manual mixing/machine mixing, compacted by wooden or cast iron rammers, curing etc., complete.		ACC/ Birla Super, Ultratech,Materials available in Market		Cft		1		1		25		5		0.3		37.5				- 0

		11		Tiles work: floor tile Providing and laying first quality ceramic tiles 300x300mm of approved colour, make and set in cement mortor, 20mm thick including pointing with tinted white cement to match the colour of tiles. Rate to include for laying tiles of approved size to the pattern as directed by the organisation including curing, acid wash etc., complete.  the rate shall include for POP coating over polythene sheet for protection of the polished floor till handing over the building.  		Vetrified/ceramic, Kajaria, Janson or Market available		Sft		1		1		25		5				125				- 0		For Class room

		12		Demolition of existing door for Classroom. Cost includes removing and stacking and dumping waste materials, labour cost etc. complete		Materials Available in Market		Sqft		1				4		7				28				- 0

		13		Block work: Providing & constructing with Concrete block masonry 230mm thick in superstructure at all levels and heights with approved quality Hallow brick of minimum crushing strength 50 kgs/sqcm, in CM 1:6 including raking the joints neatly to a depth of 12mm, curing, scaffolding, with all leads and lifts and as directed by STC Engineer in charge. etc. complete.		ACC/ Birla Super, Ultratech,Materials available in Market		Sft		1		1		4				7		28				- 0

		14		Wall Plastering: Providing the surface and plaster  the walls with cement mortar 1:6 , 15 mm thick , smooth finished to line and plumb with lime rendering at all levels rounding of corners wherever required complete with necessary scaffolding, curing etc, complete.including lead and lifts hydrating the lime for 24 hours before starting of work. (Cpmplete with Paiting)		Ultratech,ACC,Birla super, Dr. Fixit, Isoflex, Tacoma,Tremco		Sft		1		2		4				7		56				- 0

		15		Removing Existing Classroom kadapa floor tiles. Cost shall includes removing, stacking, dumping, shifting and labour cost. Etc. Complete		Materials Available in Market		Sqft		1				35		25				875				- 0

		16		Tiles work: floor tile Providing and laying first quality ceramic tiles 300x300mm of approved colour, make and set in cement mortor, 20mm thick including pointing with tinted white cement to match the colour of tiles. Rate to include for laying tiles of approved size to the pattern as directed by the organisation including curing, acid wash etc., complete.  the rate shall include for POP coating over polythene sheet for protection of the polished floor till handing over the building.  		Vetrified/ceramic, Kajaria, Janson or Market available		Sft		1		1		35		25				875				- 0		For Class room

		17		Painting (Internal and External): Providing two coats  of Apex paint (Asian Paints)  or  equivalent  ,as  per  approved  shade  &  manufacture  after  thoroughly sand papering the surfaces, removing the dust, dirt, repairing dents, holes, cracks, etc.,  applying  a  coat  of  primer  including  labour,  scaffolding  at  all  levels  with primer & putty etc., complete. (Including Ceiling)		Asian/ Birla		Sft		1				98				10		1231.24

				Inner walls				Sft		1				124				10		1240

				Deductions

				Doors				Sft		-1		3		3				7		-63

				Ventilators				Sft		-2		4		2		2				-32

				Total				Sft												2376.24				- 0

		18		Enamel Paints to Doors, Windows, Grills, Metallic Surfaces,
Walls : Providing & applying Enamel Paints to Doors, Windows, Grills, Metallic Surfaces, walls, etc. Removing, scrapping & cleaning the
existing enamel paint on doors, windows, grills, metallic surfaces, etc.
paint by scrapping, sand papering and scrubbing. Then first coat of
primer to be applied. After this necessary leveling shall be done with
putty & second primer coat shall be applied. and The enamel paint of approved shade shall be applied in minimum 3coats (finishing paint) including scaffolding, cleaning the floors, fittings, furniture's, ladders, glasses, removing of debris out of the compound etc. complete as per the instructions of the Engineer.		Asian/Birla		Sft

				Doors				Sft		1		3		3				7		63

				Ventilators				Sft		2		4		2		2				32

				Total				Sft												95				- 0

		Sub Total for Civil works																						- 0



		D		CIVIL WORKS FOR UNDER CONSTRUCTION SCHOOL BUILDING

		1		Finishing Works: Providing and completing all required finishing works for the under-construction school building, in accordance with the relevant IS Codes, applicable specifications, and instructions of the Engineer-in-Charge. The rate shall be inclusive of all materials, labour, tools, equipment, scaffolding, transportation, wastage, finishing, curing, and all other incidental charges necessary for the complete execution of the work.

The contractor shall complete the works to the required quality and workmanship standards as specified relevant IS Codes. The rate shall be quoted on a per square foot (Sq.ft) basis of the building's built-up area, based on the prevailing market rate.

The following finishing work items shall be considered under this item, including but not limited to, and shall be completed as per the requirements and instructions of the Engineer-in-Charge.				Sft		1		1		132		30				3960				- 0

		a		Paiting works including wall putty, Exterior, interior and Ceiling painting

		b		External wall painting

		c		Electrical works Including Fans, Lights, Switch boards, MCB, Panel board, etc (Electrical finishing works)

		d		Floor and skirting tiles works and Tiles work for Staircase 

		e		Door and window finishing/painting (UPVC with MS Grill)

		f		Grills and MS works painting

		g		Roof  Waterproofing works

		h		Staircase finishing

		i		Handrail painting/finishing

		Sub Total for Civil works for under construction building																						- 0



		Sub Total 																						- 0

		GST 18%																						- 0

		Grand Total																						- 0









GUDURU MANDALAM

		BAL RAKSHA BHARAT

		GUDURU MANDALAM

		R0

		Item		Description		Brands		Unit		No's		No's		L		B		D		Qty		Rate		Amount		Remarks

		A		CIVIL WORKS

		1		Providing and fixing 1 HP motor with Proper Electricity connection		Sharp/ Texmo		No's		1										1				- 0

		2		Providing and fixing SS Long body tap 		Parryware/Cera		Sft		10		1						3		30				- 0

		3		Providing and Construction of Chamber for Proper Drainage with Cement concrete blocks and Finish with proper work by cover it with slab.		Ultratech,ACC,Birla super, Dr. Fixit, Isoflex, Tacoma,Tremco		Sft		1		1		2		2				4				- 0

		4		Providing and Fixing Sink Outlet pipe		Parryware/Cera		Nos		2						 				2				- 0

		5		4" PVC pipe for drainage connection		Ashirvad		Rft		1				100						100				- 0

		6		MS door: Providing and fixing 1mm thick M.S. sheet door with frame of 40x40x6 mm angle iron and 3 mm M.S. gusset plates at the junctions and corners, all necessary fittings complete, including applying a priming coat of approved steel primer. Using M.S. angels 40x40x6 mm for diagonal braces including cost of materials, labour, usage charges of machinery complete as per specifications and as per directions of the Engineer-in- Charge.		MS Engineering works		Sft		1		2		4				7		56				- 0

		7		Water Connection: Provide proper water Connection  from motor to OHT. Cost shall include all necessary items requires for water connection(Elbow, T joint etc). All CPVC pipe lines connections and other pipe line repairs. (CPVC pipe dia=3/4"). 		Ashirvad		Rft		1				100		 		 		100				- 0

		8		Providing ACID WASH for toilet		ROFF		Ltrs		1		20								20				- 0

		9		Painting (Internal and External): Providing two coats  of Apex paint (Asian Paints)  or  equivalent  ,as  per  approved  shade  &  manufacture  after  thoroughly sand papering the surfaces, removing the dust, dirt, repairing dents, holes, cracks, etc.,  applying  a  coat  of  primer  including  labour,  scaffolding  at  all  levels  with primer & putty etc., complete. (Including Ceiling)		Asian/ Birla		Sft		1				80				10		1051.24

				Inner walls				Sft		1				152				10		1520

				Deductions

				Doors				Sft		-1		2		3				7		-42

				Ventilators				Sft		-2		2		2		2				-16

				Total				Sft												2513.24				- 0

		10		Enamel Paints to Doors, Windows, Grills, Metallic Surfaces,
Walls : Providing & applying Enamel Paints to Doors, Windows, Grills, Metallic Surfaces, walls, etc. Removing, scrapping & cleaning the
existing enamel paint on doors, windows, grills, metallic surfaces, etc.
paint by scrapping, sand papering and scrubbing. Then first coat of
primer to be applied. After this necessary leveling shall be done with
putty & second primer coat shall be applied. and The enamel paint of approved shade shall be applied in minimum 3coats (finishing paint) including scaffolding, cleaning the floors, fittings, furniture's, ladders, glasses, removing of debris out of the compound etc. complete as per the instructions of the Engineer.		Asian/Birla		Sft

				Doors				Sft		2		2		3				7		84

				Ventilators				Sft		2		2		2		2				16

				Total				Sft												100				- 0

		Sub Total for Civil works																						- 0



		Sub Total 																						- 0

		GST 18%																						- 0

		Grand Total																						- 0









PYNAPURAM

		BAL RAKSHA BHARAT

		PYNAPURAM

		R0

		Item		Description		Brands		Unit		No's		No's		L		B		D		Qty		Rate		Amount		Remarks

		A		HAND WASH STATION

		1		Excavation work: Excavation in all types of soil including dense soil,disintegrated/weathered/soft rock for  footings of Retaining walls, catchpits, Lift pits, trenches for drains, etc.,by manual means where it is not possible to excavate by machines or mechanical means including excavation for levelling, dressing the edges, all leads and lifts including back filling in layers of 150mm with watering and compaction, dewatering of both ground and surface water, removal of slurry generated while excavation and keeping the area free of water with necessary shoring, strutting, required for keeping earth in position etc. Rate to include disposing the excess earth and spreading in layers to the required levels within the site wherever specified and carting away outside the site to the designated areas identified by the local authorities.		Materials available in Market		Cft		1		1		12		3		0.75		27				- 0

		2		Block work: Providing & constructing with Concrete block masonry 150mm thick in superstructure at all levels and heights with approved quality Hallow brick of minimum crushing strength 50 kgs/sqcm, in CM 1:6 including raking the joints neatly to a depth of 12mm, curing, scaffolding, with all leads and lifts and as directed by STC Engineer in charge. etc. complete.		ACC/ Birla Super, Ultratech,Materials available in Market		Sft		1		1		17				3		51				- 0

		3		Wall Plastering: Providing the surface and plaster  the walls with cement mortar 1:6 , 15 mm thick , smooth finished to line and plumb with lime rendering at all levels rounding of corners wherever required complete with necessary scaffolding, curing etc, complete.including lead and lifts hydrating the lime for 24 hours before starting of work.		Ultratech,ACC,Birla super, Dr. Fixit, Isoflex, Tacoma,Tremco		Sft		1		1		10				3		30				- 0

		4		Tiles work: Providing  &  laying  first  quality  Vitrified Tiles  of   approved  colour, make  300x 400  Glossy finish set  in cement mortar bed 1:4, 20mm thick including pointing with tinted white cement to  match the colour of  tiles. Rate to include for laying tiles of approved size to the pattern as directed by  the STC Engineer or STC Employees including curing, acid wash etc., complete. 		Vetrified, Kajaria, Cera, Janson or Market available		Sft		1				32		 		3		96				- 0

		5		Water Connection: Provide proper water Connection  from OHT to Hand wash area. Cost shall include all necessary items requires for water connection(Elbow, T joint etc). All CPVC pipe lines connections and other pipe line repairs. (CPVC pipe dia=3/4"). (Make proper drainage connection to flow waste water from hand wash station to drainage line or UGD)		Ashirvad		Rft		1				200						200				- 0

		6		4" PVC pipe for drainage connection		Ashirvad		Rft		1				50						50				- 0

		7		Brass Tee (3/4x3/4x3/4)		Ashirvad		Nos		1				6						6				- 0

		8		SS Long body tap		Parryware/Cera		Nos		1		6								6				- 0

		9		Reinforcement steel: Supplying  and  fixing  reinforcement  for  R.C.C.  In  all  items  works  including transporting, decoiling, cutting, straightening bending and placing in position at all levels and binding with approved gauge binding wire. The rate shall include cost  of  binding  wire, chairs,  spacers  which  will not  be measured  separately  for payment.  Quantity of steel as per drawing and with authorized overlaps only shall be measured and paid for.  High yield strength deformed bars conforming to Yst 415 N/mm2 as per IS 1786 		Appollo/Jindal/TATA		Kg		0.12				48						5.76				- 0

		10		Plain cement concrete: Providing and laying plain cement concrete(PCC) 1:4:8 for flooring with smooth finishing using graded granite aggregate of 12 mm and down size, provide thickness upto 4" and it including matrials, labours, manual mixing/machine mixing, compacted by wooden or cast iron rammers, curing etc., complete.		ACC/ Birla Super, Ultratech,Materials available in Market		Cft		1				24		2		0.5		24				- 0

		11		Safety Grill for Hand wash Station: Providing and fixing safety grill for hand wash with all necesssary fixtures and complete.,		Materials available in Market		Sft		1		120								120				- 0

		Sub Total for Hand Wash Station																						- 0



		B		Civil works

		1		Providing and fixing 1 HP motor with Proper Electricity connection		Sharp/ Texmo		No's		1										1				- 0

		2		Providing and fixing suitable RCC/PCC drainage cover slabs over existing open drainage channels around the school premises to facilitate safe pedestrian access and prevent accidental falls, including cleaning of drains, proper alignment and levelling of cover slabs, maintaining drainage flow and providing access for future maintenance. Also, providing a child-friendly hand wash station with suitable platform, water taps, water supply and wastewater drainage connections, including all required plumbing fittings, civil works, finishing, labour, materials, tools and equipment, complete as per approved specifications and instructions of the Engineer-in-Charge.		Ultratech,ACC,Birla super, 		Sqft		10				4		3				120				- 0

		3		Providing and Construction of Chamber for Proper Drainage with Cement concrete blocks and Finish with proper work by cover it with slab.		Ultratech,ACC,Birla super, Dr. Fixit, Isoflex, Tacoma,Tremco		Sft		1		1		2		2				4				- 0

		4		Toilet water closet: Removing existing IWC Petite EWC Set
C0287*/C0288* (S/P) Trap Petite EWC (515 X 360 X 405mm) with E8309 Petite Plus Seat and Cover and Flush tank Standard E8297with Long Bend Pipe (685mm) and Providing and fixing water closet squatting pan (Indian type W.C. pan ) with 100 mm sand cast Iron P or S trap, Complete with all fittings and fixtures complete, including cutting and making good the walls and floors wherever required.		Parryware		No's		1		1								1				- 0

		5		Providing ACID WASH for toilet		ROFF		Ltrs		1		20								20				- 0

		6		Ceiling Plastering: Removing existing damaged cieling plaster and Providing the surface and plaster the ceiling with Fosroc Waterproof chemical with cement mortar 1:6 , 15 mm thick, smooth finished to line and plumb with lime rendering at all levels rounding of corners wherever required complete with necessary scaffolding, curing etc, complete.including lead and lifts hydrating the lime for 24 hours before starting of work.		Ultratech,ACC,Birla super, Dr. Fixit, Isoflex, Tacoma,Tremco/FOSROC		Sft		1		6		18		9				972				- 0

		7		Water proofing the Roof slab : The first method consists of water proofing by surface method of average thickness 2" with waterproof admixture as per manufacturer's specification approved by Consultants with a minimum Guarantee period of 10 years. Cost to include – Cement slurry with waterproofing compound applied over the surface after cleaning the surface - Laying of brick coba to necessary gradient and joints filled with CM 1:4 with water proofing compoundCost to include the treatment along parapet,treatment to construction joints,pressure grouting of damp areas using cementitious grouting etc, and no extra measurements shall be accounted for the parapet treatment with Curing the entire surface for  a minimum  period of seven days.  (CLEANING AND CHEMICAL COATING)		Birla Opus ALLDRY/JSW I BLOCK WATERSTOP  ROOF COAT		Sft		1		7		18		9				1134				- 0

		8		Painting (Internal and External): Providing two coats  of Apex paint (Asian Paints)  or  equivalent  ,as  per  approved  shade  &  manufacture  after  thoroughly sand papering the surfaces, removing the dust, dirt, repairing dents, holes, cracks, etc.,  applying  a  coat  of  primer  including  labour,  scaffolding  at  all  levels  with primer & putty etc., complete. (Including Ceiling)		Asian/ Birla		Sft		1				80				10		1051.24

				Inner walls				Sft		1				152				10		1520

				Deductions

				Doors				Sft		-1		2		3				7		-42

				Ventilators				Sft		-2		2		2		2				-16

				Total				Sft												2513.24				- 0

		9		Enamel Paints to Doors, Windows, Grills, Metallic Surfaces,
Walls : Providing & applying Enamel Paints to Doors, Windows, Grills, Metallic Surfaces, walls, etc. Removing, scrapping & cleaning the
existing enamel paint on doors, windows, grills, metallic surfaces, etc.
paint by scrapping, sand papering and scrubbing. Then first coat of
primer to be applied. After this necessary leveling shall be done with
putty & second primer coat shall be applied. and The enamel paint of approved shade shall be applied in minimum 3coats (finishing paint) including scaffolding, cleaning the floors, fittings, furniture's, ladders, glasses, removing of debris out of the compound etc. complete as per the instructions of the Engineer.		Asian/Birla		Sft

				Doors				Sft		2		2		3				7		84

				Ventilators				Sft		2		2		2		2				16

				Total				Sft												100				- 0

		Sub Total for Civil works in Girls toilet																						- 0



		Sub Total 																						- 0

		GST 18%																						- 0

		Grand Total																						- 0









VARAKAVIPUDI

		BAL RAKSHA BHARAT

		VARAKAVIPUDI

		R0

		Item		Description		Brands		Unit		No's		No's		L		B		D		Qty		Rate		Amount		Remarks

		A		HAND WASH STATION

		1		Excavation work: Excavation in all types of soil including dense soil,disintegrated/weathered/soft rock for  footings of Retaining walls, catchpits, Lift pits, trenches for drains, etc.,by manual means where it is not possible to excavate by machines or mechanical means including excavation for levelling, dressing the edges, all leads and lifts including back filling in layers of 150mm with watering and compaction, dewatering of both ground and surface water, removal of slurry generated while excavation and keeping the area free of water with necessary shoring, strutting, required for keeping earth in position etc. Rate to include disposing the excess earth and spreading in layers to the required levels within the site wherever specified and carting away outside the site to the designated areas identified by the local authorities.		Materials available in Market		Cft		1		1		20		3		0.75		45				- 0

		2		Block work: Providing & constructing with Concrete block masonry 150mm thick in superstructure at all levels and heights with approved quality Hallow brick of minimum crushing strength 50 kgs/sqcm, in CM 1:6 including raking the joints neatly to a depth of 12mm, curing, scaffolding, with all leads and lifts and as directed by STC Engineer in charge. etc. complete.		ACC/ Birla Super, Ultratech,Materials available in Market		Sft		1		1		80				3		240				- 0

		3		Wall Plastering: Providing the surface and plaster  the walls with cement mortar 1:6 , 15 mm thick , smooth finished to line and plumb with lime rendering at all levels rounding of corners wherever required complete with necessary scaffolding, curing etc, complete.including lead and lifts hydrating the lime for 24 hours before starting of work.		Ultratech,ACC,Birla super, Dr. Fixit, Isoflex, Tacoma,Tremco		Sft		1		1		120				3		360				- 0

		4		Tiles work: Providing  &  laying  first  quality  Vitrified Tiles  of   approved  colour, make  300x 400  Glossy finish set  in cement mortar bed 1:4, 20mm thick including pointing with tinted white cement to  match the colour of  tiles. Rate to include for laying tiles of approved size to the pattern as directed by  the STC Engineer or STC Employees including curing, acid wash etc., complete. 		Vetrified, Kajaria, Cera, Janson or Market available		Sft		1				120		 		3		360				- 0

		5		Water Connection: Provide proper water Connection  from OHT to Hand wash area. Cost shall include all necessary items requires for water connection(Elbow, T joint etc). All CPVC pipe lines connections and other pipe line repairs. (CPVC pipe dia=3/4"). (Make proper drainage connection to flow waste water from hand wash station to drainage line or UGD)		Ashirvad		Rft		1				50						50				- 0		Inlcuding RO Connection

		6		4" PVC pipe for drainage connection		Ashirvad		Rft		1				100						100				- 0

		7		Brass Tee (3/4x3/4x3/4)		Ashirvad		Nos		1				10						10				- 0

		8		SS Long body tap 		Parryware/Cera		Nos		1		10								10				- 0

		9		Reinforcement steel: Supplying  and  fixing  reinforcement  for  R.C.C.  In  all  items  works  including transporting, decoiling, cutting, straightening bending and placing in position at all levels and binding with approved gauge binding wire. The rate shall include cost  of  binding  wire, chairs,  spacers  which  will not  be measured  separately  for payment.  Quantity of steel as per drawing and with authorized overlaps only shall be measured and paid for.  High yield strength deformed bars conforming to Yst 415 N/mm2 as per IS 1786 		Appollo/Jindal/TATA		Kg		0.20				120						24				- 0

		10		Plain cement concrete: Providing and laying plain cement concrete(PCC) 1:4:8 for flooring with smooth finishing using graded granite aggregate of 12 mm and down size, provide thickness upto 4" and it including matrials, labours, manual mixing/machine mixing, compacted by wooden or cast iron rammers, curing etc., complete.		ACC/ Birla Super, Ultratech,Materials available in Market		Cft		1				40		2		0.5		40				- 0

		Sub Total for Hand Wash Station																						- 0



		B		Civil works for toilet

		1		WPC Door: Providing and fixing 30mm Solid WPC Door of density 0.55 with frame for toilet with all necessary fixtures with Door frame and provide and safety lock. Cost shall includes all labour cost, material cost, fixing charges, etc.                                                                           		Materials available in Market		Sft		1		1		3				6		18				- 0

		2		SS Long body tap 		Parryware/Cera		Nos		1		20								20				- 0

		3		Providing 3" PVC pipe for drainage connection		Ashirvad		No's		1				100						100				- 0

		4		Providing ACID WASH for toilet		ROFF		Ltrs		1		20								20				- 0

		5		Water proofing the Roof slab : The first method consists of water proofing by surface method of average thickness 2" with waterproof admixture as per manufacturer's specification approved by Consultants with a minimum Guarantee period of 10 years. Cost to include – Cement slurry with waterproofing compound applied over the surface after cleaning the surface - Laying of brick coba to necessary gradient and joints filled with CM 1:4 with water proofing compoundCost to include the treatment along parapet,treatment to construction joints,pressure grouting of damp areas using cementitious grouting etc, and no extra measurements shall be accounted for the parapet treatment with Curing the entire surface for  a minimum  period of seven days.  (CLEANING AND CHEMICAL COATING)		Birla Opus ALLDRY/JSW I BLOCK WATERSTOP  ROOF COAT		Sft		1				80		30				2400				- 0

		6		Providing and Cleaning Septic tank				Nos		2										2				- 0

		7		Providing 3 no's precast RCC rings for burning wastage				Nos				3								3				- 0

		8		MS Safety Gril for Corridor area: Providing and fixing 1"x1" square MS welded wire mesh with sides arounds L Channel welded with mesh compolete with all necessary fixture and finishing the same with one coat of zinc cromate primer and two coats of enamel paint of approved make. The M.S. Grill is with following members: (a) 25x6mm Brite Flat as vertical member; (b) 10mm square brite horizontal bar punched through the flat Rate shall includes material cost, labour cost, cutting cahrges shifting, welding etc., Complete as per the STC engineer in charge 		Materials available in Market		Sft		1		1		70				5		350				- 0

		9		Electrical work		 		 		 										  				 

		a		Switch board with 16amp switches for light and fan		Havells/Cona/Schneider		Lumspum		4		2								8				- 0

		b		MCB		Havells/Cona/Schneider		No's		4		1		 						4				- 0

		c		Power cable for electricity		Havells/Cona/Schneider		Rft		4		200								800				- 0

		d		PVC cable pipe with necessary fixtures		Ashirvad		Rft		4		120								480				- 0

		e		ceiling fan		crompton/havelles		No's		10		2		 						20				- 0

		f		LED Tube light 		crompton/havelles		no's		10		2								20				- 0

		10		Ceiling Plastering:  Removing and Providing the surface and plaster the ceiling with Fosroc Waterproof chemical with cement mortar 1:6 , 15 mm thick, smooth finished to line and plumb with lime rendering at all levels rounding of corners wherever required complete with necessary scaffolding, curing etc, complete.including lead and lifts hydrating the lime for 24 hours before starting of work.		Ultratech,ACC,Birla super, Dr. Fixit, Isoflex, Tacoma,Tremco/FOSROC		Sft		1		1		80		15				1200				- 0

		11		MS door: Providing and fixing 1mm thick M.S. sheet door with frame of 40x40x6 mm angle iron and 3 mm M.S. gusset plates at the junctions and corners, all necessary fittings complete, including applying a priming coat of approved steel primer. Using M.S. angels 40x40x6 mm for diagonal braces including cost of materials, labour, usage charges of machinery complete as per specifications and as per directions of the Engineer-in- Charge.		MS Engineering works		Sft		1		1		4				7		28				- 0

		12		Wall Plastering: Providing the surface and plaster  the walls with cement mortar 1:6 , 15 mm thick , smooth finished to line and plumb with lime rendering at all levels rounding of corners wherever required complete with necessary scaffolding, curing etc, complete.including lead and lifts hydrating the lime for 24 hours before starting of work.		Ultratech,ACC,Birla super, 		Sft		1		1		100		10				1000				- 0		Near Door corners

		13		Water Connection: Provide proper water Connection  from water ATM to School with 3 Taps. Cost shall include all necessary items requires for water connection(Elbow, T joint etc). All CPVC pipe lines connections and other pipe line repairs. (CPVC pipe dia=3/4"). 		Ashirvad		Rft		1				500		 		 		500				- 0

		14		Painting (Internal and External): Providing two coats  of Apex paint (Asian Paints)  or  equivalent  ,as  per  approved  shade  &  manufacture  after  thoroughly sand papering the surfaces, removing the dust, dirt, repairing dents, holes, cracks, etc.,  applying  a  coat  of  primer  including  labour,  scaffolding  at  all  levels  with primer & putty etc., complete. (Including Ceiling)		Asian, Birla Opus, JSW paints		Sft		1				1800				11		19800				- 0

		Sub Total for Civil works in Girls toilet																						- 0



		Sub Total 																						- 0

		GST 18%																						- 0

		Grand Total																						- 0
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		Item		Description		Brands		Unit		No's		No's		L		B		D		Qty		Rate		Amount		Remarks

		A		Civil works for toilet

		1		Septic tank: Construction of new septic tank  using 6 no's precast RCC rings, with caps(self casted RCC cap with 50.8 mm thick) drainge line from toilet to septic tank to make it functional and complete with filling 40mm jelly around the rings till 4feet height.  (4ft dia, 7 ft depth, 1ft Above GL) (Scope includes Excavations, Backfill, civil works (1 cement bag), plumbing works,labour charges, req material, req machinary, site cleaning and all other meterial,manpower requied to make it functional).		Materials available in Market		No's		2										2				- 0

		2		Providing and Cleaning Septic tank				Nos		1										1				- 0

		3		Providing 4" PVC pipe for drainage connection		Ashirvad		No's		1				100						100				- 0

		4		Providing ACID WASH for toilet		ROFF		Ltrs		1		20								20				- 0

		5		MS door: Providing and fixing 1mm thick M.S. sheet door with frame of 40x40x6 mm angle iron and 3 mm M.S. gusset plates at the junctions and corners, all necessary fittings complete, including applying a priming coat of approved steel primer. Using M.S. angels 40x40x6 mm for diagonal braces including cost of materials, labour, usage charges of machinery complete as per specifications and as per directions of the Engineer-in- Charge.		MS Engineering works		Sft		1		20		3				7		420				- 0

		6		MS Safety Gril for Corridor area: Providing and fixing 1"x1" square MS welded wire mesh with sides arounds L Channel welded with mesh compolete with all necessary fixture and finishing the same with one coat of zinc cromate primer and two coats of enamel paint of approved make. The M.S. Grill is with following members: (a) 25x6mm Brite Flat as vertical member; (b) 10mm square brite horizontal bar punched through the flat Rate shall includes material cost, labour cost, cutting cahrges shifting, welding etc., Complete as per the STC engineer in charge 		Materials available in Market		Sft		1		1		70				5		350				- 0

		7		Electrical work		 		 		 										  				 

		a		Switch board with 16amp switches for light and fan		Havells/Cona/Schneider		Lumspum		4		2								8				- 0

		b		MCB		Havells/Cona/Schneider		No's		4		1		 						4				- 0

		c		Power cable for electricity		Havells/Cona/Schneider		Rft		4		200								800				- 0

		d		PVC cable pipe with necessary fixtures		Ashirvad		Rft		4		120								480				- 0

		e		ceiling fan		crompton/havelles		No's		10		2		 						20				- 0

		f		LED Tube light 		crompton/havelles		no's		10		2								20				- 0

		8		Ceiling Plastering:  Providing the surface and plaster the ceiling with Fosroc Waterproof chemical with cement mortar 1:6 , 15 mm thick, smooth finished to line and plumb with lime rendering at all levels rounding of corners wherever required complete with necessary scaffolding, curing etc, complete.including lead and lifts hydrating the lime for 24 hours before starting of work.		Ultratech,ACC,Birla super, Dr. Fixit, Isoflex, Tacoma,Tremco/FOSROC		Sft		1		1		80		15				1200				- 0

		9		MS door: Providing and fixing 1mm thick M.S. sheet door with frame of 40x40x6 mm angle iron and 3 mm M.S. gusset plates at the junctions and corners, all necessary fittings complete, including applying a priming coat of approved steel primer. Using M.S. angels 40x40x6 mm for diagonal braces including cost of materials, labour, usage charges of machinery complete as per specifications and as per directions of the Engineer-in- Charge.		MS Engineering works		Sft		1		1		4				7		28				- 0

		10		Wall Plastering: Providing the surface and plaster  the walls with cement mortar 1:6 , 15 mm thick , smooth finished to line and plumb with lime rendering at all levels rounding of corners wherever required complete with necessary scaffolding, curing etc, complete.including lead and lifts hydrating the lime for 24 hours before starting of work.		Ultratech,ACC,Birla super, 		Sft		1		1		100		10				1000				- 0		Near Door corners

		11		Water Connection: Provide proper water Connection  from water ATM to School with 3 Taps. Cost shall include all necessary items requires for water connection(Elbow, T joint etc). All CPVC pipe lines connections and other pipe line repairs. (CPVC pipe dia=3/4"). 		Ashirvad		Rft		1				500		 		 		500				- 0

		12		Block work: Providing & constructing with Concrete block masonry 200mm thick in superstructure at all levels and heights with approved quality Hallow brick of minimum crushing strength 50 kgs/sqcm, in CM 1:6 including raking the joints neatly to a depth of 12mm, curing, scaffolding, with all leads and lifts and as directed by STC Engineer in charge. etc. complete.		ACC/ Birla Super, Ultratech,Materials available in Market		Sft		1				40		 		6		240				- 0

		13		Wall Plastering: Providing the surface and plaster  the walls with cement mortar 1:6 , 15 mm thick , smooth finished to line and plumb with lime rendering at all levels rounding of corners wherever required complete with necessary scaffolding, curing etc, complete.including lead and lifts hydrating the lime for 24 hours before starting of work.		Ultratech,ACC,Birla super, Dr. Fixit, Isoflex, Tacoma,Tremco		Sft		2				40				6		480				- 0

		14		Painting: Providing one primer coat  and two coats  of Apex  Exterior  paint (Asian Paints)  or  equivalent  ,as  per  approved  shade  &  manufacture  after  thoroughly sand papering the surfaces, removing the dust, dirt, repairing dents, holes, cracks, etc.,  applying  a  coat  of  primer  including  labour,  scaffolding  at  all  levels  with primer & putty etc., complete 		Asian/ Birla		Sft		2				40				6		480				- 0

		15		Plain cement concrete: Providing and laying plain cement concrete(PCC) 1:4:8 for flooring with smooth finishing using graded granite aggregate of 12 mm and down size, provide thickness upto 4" and it including matrials, labours, manual mixing/machine mixing, compacted by wooden or cast iron rammers, curing etc., complete.		ACC/ Birla Super, Ultratech,Materials available in Market		Cft		1		1		30		10		0.3		90				- 0

		16		Painting (Internal and External): Providing two coats  of Apex paint (Asian Paints)  or  equivalent, and Enamel paint for Doors as  per  approved  shade  &  manufacture  after  thoroughly sand papering the surfaces, removing the dust, dirt, repairing dents, holes, cracks, etc.,  applying  a  coat  of  primer  including  labour,  scaffolding  at  all  levels  with primer & putty etc., complete. (Including Ceiling)		Asian, Birla Opus, JSW paints		Sft		3				150				11		4950				- 0

		Sub Total for Civil works in Girls toilet																						- 0



		B		CIVIL WORKS FOR UNDER CONSTRUCTION SCHOOL BUILDING (Kitchen)

		1		Finishing Works: Providing and completing all required finishing works for the under-construction school building, in accordance with the relevant IS Codes, applicable specifications, and instructions of the Engineer-in-Charge. The rate shall be inclusive of all materials, labour, tools, equipment, scaffolding, transportation, wastage, finishing, curing, and all other incidental charges necessary for the complete execution of the work.

The contractor shall complete the works to the required quality and workmanship standards as specified relevant IS Codes. The rate shall be quoted on a per square foot (Sq.ft) basis of the building's built-up area, based on the prevailing market rate.

The following finishing work items shall be considered under this item, including but not limited to, and shall be completed as per the requirements and instructions of the Engineer-in-Charge.				Sft		1		1		23		20				460				- 0

		a		Paiting works including wall putty, Exterior, interior and Ceiling painting

		b		External wall painting

		c		Electrical works Including Fans, Lights, Switch boards, MCB, Panel board, etc (Electrical finishing works)

		d		Floor and skirting tiles works 

		e		Iron Door and window finishing/painting (UPVC with MS Grill)

		f		Grills and MS works painting

		g		Kitchen Shelves

		h		Roof  Waterproofing works

		Sub Total for Civil works for under construction building																						- 0



		Sub Total 																						- 0

		GST 18%																						- 0

		Grand Total																						- 0
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